**IX-DVM**

**FEATURES**

* Small form factor for mullion mounting
* Contactless call sensor
* SIP 2.0 compliant
* 720p HD, wide dynamic range camera
* White LED for low-light illumination
* ONVIF Profile S compliant
* Slot for microSD™ card (not provided by Aiphone)
* One contact output
* One trigger input
* 802.3af PoE compliant
* Certified [DevConnect Technology Partner](https://www.aiphone.com/home/products/avaya-solution-partner%22%20%5Ct%20%22_blank) with Avaya IP Office™, Avaya Aura® Communication Manager.
* Manufactured in a TAA compliant country

**SPECS**

Power Source:

PoE (IEEE 802.3af class 0)

Power Draw:

4.6W max.

Camera:

720p HD, wide dynamic range

Camera angle:

Approx. 170° horizontal

Class 1 laser:

This product incorporates a Class 1 laser. (transmissions conform with IEC 60825-1:2014)

Relay Output Output Method:

Form C dry contact (N/O or N/C)

Contact Rating:

24V AC, 1A (resistive load) 24V DC, 1A (resistive load)

Audio Codec:

G.711 (μ-law, A law), G.722

Video Codec:

H.264/AVC, motion JPEG

Protocols:

IPv4, IPv6, TCP, UDP, SIP, HTTP, HTTPS, RTSP, RTP, RTCP, IGMP, MLD, SMTP, FTP, DHCP, NTP, DNS

Port Security:

IEEE 802.1X

Operating Temp:

-40° ~ 140°F (-40° ~ 60°C)

Protection:

IP54, IK07

Dimensions:

1-7/8" W x 1-5/16" L x 6-7/8" H